<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="60.96" y1="0" x2="60.96" y2="83.82" width="0" layer="20"/>
<wire x1="60.96" y1="83.82" x2="0" y2="83.82" width="0" layer="20"/>
<wire x1="0" y1="83.82" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="60.96" y2="0" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>D9</text>
<text>G</text>
<text>+3</text>
<text>-</text>
<text>TH</text>
<text>-</text>
<text>PCR</text>
<text>THERMOCYCLER</text>
<text>UZAM &amp; WAJID</text>
</plain>
<libraries>
<library name="Atmel_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="QFP80P1200X1200X120-44N">
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="USB_MINIB">
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ng">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-amp-quick">
<description>&lt;b&gt;AMP Connectors, Type QUICK&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="02P">
<description>&lt;b&gt;AMP QUICK CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Atmel_By_element14_Batch_1" package="QFP80P1200X1200X120-44N" value="ATMEGA32U4-AU">
<attribute name="MPN" value="ATMEGA32U4-AU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1748525"/>
<attribute name="OC_NEWARK" value="26R5633"/>
<attribute name="PACKAGE" value="TQFP-44"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB_UPLOAD" library="fab" package="USB_MINIB" value="USB_MINIB">
<attribute name="NAME"/>
</element>
<element name="C7" library="fab" package="C1206FAB" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="fab" package="C1206FAB" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fab" package="R1206FAB" value="10K"/>
<element name="C10" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="ng" package="1206" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D13_LED" library="ng" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="fab" package="R1206FAB" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB_LED" library="ng" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="ng" package="1206" value="499"/>
<element name="TX_LED" library="ng" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="ng" package="1206" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX_LED" library="ng" package="1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="ng" package="1206" value="499">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X02_NO_SILK" value=""/>
<element name="C11" library="fab" package="C1206FAB" value="10uF"/>
<element name="5-3.3V" library="fab" package="SOT223" value="">
<attribute name="PROD_ID" value="VREG-08170"/>
</element>
<element name="C12" library="fab" package="C1206FAB" value="10uF"/>
<element name="C13" library="fab" package="C1206FAB" value="10uF"/>
<element name="JP1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="R13" library="fab" package="R1206FAB" value="100K"/>
<element name="SL2" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="PROD_ID" value="XXX-00000"/>
<attribute name="VALUE" value="455-1750-1-ND"/>
</element>
<element name="SL1" library="con-amp-quick" package="02P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X05" value=""/>
<element name="POWER-PINS" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
<element name="THERM-100K" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="Q1" library="adafruit" package="HC49/S" value="">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PROG_3X2PTH"/>
<element name="R9" library="adafruit" package="0204/7" value="0"/>
<element name="R10" library="adafruit" package="0204/7" value="0"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="23"/>
<contactref element="U1" pad="35"/>
<contactref element="U1" pad="43"/>
<contactref element="U1" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="USB_UPLOAD" pad="GND"/>
<contactref element="C8" pad="2"/>
<contactref element="RESET" pad="2"/>
<contactref element="RESET" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="D13_LED" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="USB_UPLOAD" pad="SHIELD@2"/>
<contactref element="USB_UPLOAD" pad="SHIELD@1"/>
<contactref element="USB_UPLOAD" pad="SHIELD@3"/>
<contactref element="USB_UPLOAD" pad="SHIELD@4"/>
<contactref element="USB_LED" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="5-3.3V" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="JP5" pad="7"/>
<contactref element="JP2" pad="8"/>
<contactref element="R13" pad="1"/>
<contactref element="SL2" pad="2"/>
<contactref element="SL1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="POWER-PINS" pad="2"/>
<contactref element="POWER-PINS" pad="3"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="USB_UPLOAD" pad="VBUS"/>
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="44"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="R8" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="5-3.3V" pad="3"/>
<contactref element="J6" pad="1"/>
<contactref element="SL2" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="POWER-PINS" pad="4"/>
<contactref element="THERM-100K" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="XTAL1">
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="17"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="XTAL2">
<contactref element="C6" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="D14">
<contactref element="U1" pad="8"/>
</signal>
<signal name="D15">
<contactref element="U1" pad="9"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="D16">
<contactref element="U1" pad="10"/>
<contactref element="J2" pad="4"/>
<contactref element="R9" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="D17">
<contactref element="U1" pad="11"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="D13">
<contactref element="U1" pad="32"/>
<contactref element="R4" pad="1"/>
<contactref element="JP5" pad="6"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="TXLED">
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$1">
<contactref element="USB_UPLOAD" pad="D-"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="USB_UPLOAD" pad="D+"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="D-">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="D+">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="UCAP">
<contactref element="C8" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="13"/>
<contactref element="RESET" pad="4"/>
<contactref element="RESET" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="POWER-PINS" pad="6"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="AREF">
<contactref element="C10" pad="1"/>
<contactref element="U1" pad="42"/>
<contactref element="JP5" pad="8"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="D13_LED" pad="1"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="19"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="D11">
<contactref element="U1" pad="12"/>
<contactref element="JP5" pad="4"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="18"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="USB_LED" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="20"/>
<contactref element="RX_LED" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="21"/>
<contactref element="TX_LED" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="25"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="D12">
<contactref element="U1" pad="26"/>
<contactref element="JP5" pad="5"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="27"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="28"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="29"/>
<contactref element="JP5" pad="2"/>
<contactref element="SL2" pad="3"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="30"/>
<contactref element="JP5" pad="3"/>
<contactref element="SL1" pad="1"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="31"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="A0">
<contactref element="U1" pad="36"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="37"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="38"/>
<contactref element="J1" pad="3"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="39"/>
<contactref element="J1" pad="5"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="40"/>
<contactref element="J1" pad="4"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="41"/>
<contactref element="R13" pad="2"/>
<contactref element="J3" pad="6"/>
<contactref element="THERM-100K" pad="2"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="TX_LED" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$4">
<contactref element="RX_LED" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="5-3.3V" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="5-3.3V" pad="4"/>
<contactref element="JP2" pad="6"/>
<contactref element="POWER-PINS" pad="5"/>
</signal>
<signal name="1">
<contactref element="U1" pad="33"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$11">
</signal>
<signal name="N$12">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="VIN">
<contactref element="POWER-PINS" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
